|  |  |
| --- | --- |
| Vortex (3) | Working fine |
| pH-meter (1) | Calibrated and working fine |
| Hood | Working fine; few hoods need repair and Josh is taking care of those |
| Vacuum pump (1) | Working fine |
| Microtube rotors (2) | Working fine |
| Rotors (2) | Working fine |
| Micropumps (6) | Working fine |
| Heat Press | Working fine |
| Balance | Working fine |
| Chemigenius ECL system | Working fine |
| G1Box ECL system | Working fine |
| Sonicators (2) | Working fine: water level not maintained |
| Fiber optic illuminator | Working fine |
| Form1+ 3D printer | Under repair |
| Draken 3D | Installed; testing in progress |
| UPLC | Working fine |
| Refrigerated centrifuge | Working fine |
| Temperature controlled shaker | Working fine |
| CHI660 | Working fine |
| CHI1040B | Working fine |
| CHI1030 | Working fine |
| CHI1040A | Working fine |
| CHI1040C | Working fine |
| AFM | Working fine; few tips left |
| Vaccum Oven | Working as an oven only; gasket is not sealing properly; company discontinued this product |
| Eye Stations | Working fine |
| No spillage or broken glass reported |  |